**USAGE NOTE:**

**Choose YES or NO. An “R” added beside the checkbox identifies information that is required to be included in procedure. Make sure this information gets added to the procedure prior to submittal for approval.**

Company:

Procedure:

Revision:

| **“MINIMUM” (SHALL) ATTRIBUTES REQUIRED** | | | | |
| --- | --- | --- | --- | --- |
| **Has the subject information been included in the procedure?** | | **SUBJECT** | **TP271 Para.** | **SNT-TC-1A**  **2001**  **Para.** |
| **Procedure Approval** | | | | |
| **YES** | **NO** |  | | |
| R |  | Certification statement signed by the Level III Examiner. | 1.7.1 | N/A |
| R |  | Level III Examiner’s approval/signature | 1.7.3 | 5.4 |
| **Personnel Qualification** | | | | |
| **YES** | **NO** |  | | |
| R |  | Levels I, II and III. | 1.5.5, 1.5.6, 1.5.7 & 1.6 | 4.3 |
| R |  | Training, Experience and Education | 1.6 & 1.6.1.1 | 6.3.1 & 6.3.2 |
| R |  | NDT personnel certified in accordance with MIL-STD-410 (NAS-410 not allowed) and 250-1500-1. | 1.6 & 1.6.5 | N/A |
| **Examination Grades** | | | | |
| **YES** | **NO** |  | | |
| R |  | Levels I and II. | 1.6 | 8.1 |
| R |  | Level III. | 1.6 & 1.6.1 |
| **Vision Tests** | | | | |
| **YES** | **NO** |  | | |
| R |  | Near Vision Acuity (Jaeger J-1). | 1.6.6 | 8.2.1 |
| R |  | Color Contrast Differentiation. | 8.2.2 |
| R |  | Natural or Corrected Aids Used | 8.2.1 |
| **Examinations (Levels I and II)** | | | | |
| **YES** | **NO** |  | | |
| R |  | General – Minimum 40 Questions. | 1.6 | 8.3 |
| R |  | Specific – Minimum 20 Questions. | 8.4 |
| R |  | Practical – Minimum 10 Check Points – Flawed Test Samples. | 8.5 |

|  |  |  |  |  |
| --- | --- | --- | --- | --- |
| **Examinations (Level III)** | | | | |
| **YES** | **NO** |  | | |
| R |  | Administered by Employing Activity, national ASNT or Other Outside Agency | 1.6 & 1.6.1 | 8.8 & 8.8.4 |
| R |  | Basic – Minimum 55 Questions. | 1.6 | 8.8.1 & 8.8.4 |
| R |  | Method – Minimum 65 Questions. | 8.8.2 & 8.8.4 |
| R |  | Specific – Minimum 20 Questions. | 8.8.3 |
| **Re-Examination** | | | | |
| **YES** | **NO** |  | | |
| R |  | Wait at least 30 days, or evidence of additional training. | 1.6 | 8.9 |
| **Responsibility for Certification** | | | | |
| **YES** | **NO** |  | | |
| R |  | By Employer for all NDT Levels. | 1.6.2 | 9.1 & 9.4 |
| R |  | Certifications are none transferable to another activity. | 1.6.8 | 13.2 |
| **Personnel Certification Records** | | | | |
| **YES** | **NO** |  | | |
| R |  | Maintain individual records. | 1.6.7 | 9.4 |
| R |  | Training and experience. |
| R |  | Examinations (results can be correlated to exam or master copy of exams). |
| R |  | Vision test record noting corrective aids used. |
| R |  | Maintenance (Current and preceding certification period). |

|  |  |  |  |  |
| --- | --- | --- | --- | --- |
| **Recertification** | | | | |
| **YES** | | **NO** |  | | |
| R | |  | Levels I and II: By examination at intervals not greater than three (3) years. | 1.6.3 | 8.7.2, 8.8.3.2 & 12.0 |
| R | |  | Level III: By examination at intervals not greater than five (5) years. |
| R | |  | Re-examination shall be as comprehensive as that employed in the initial certification. | N/A |
| R | |  | Alternate certifications (i.e., MIL-STDs-410 & 2132, or NAVSEA 250-1500-1) | 1.6. & 1.6.4 |
| R | |  | Personnel who perform NDT shall be recertified by an operational (practical) examination if the personnel have not performed tests in the method in which certification is held for a period of nine (9) months. | 1.6.3 |
| **Technical Performance Evaluation (TPE)** | | | | | |
| **YES** | | **NO** |  | | |
| R | |  | Periodically, TPE (Practical examination) of Levels I & II personnel shall be evaluated and documented by a NDT Level III. | 1.6 | 10.2 |
| **Interrupted Service** | | | | | |
| **YES** | | **NO** |  | | |
| R | |  | Procedure shall include rules covering the types and duration of interrupted service. | 1.6 | 11.1 |
| R | |  | Procedure shall specify the requirements for re-examination and/or recertification for the interrupted service. | 11.2 |
| **Termination** | | | | | |
| **YES** | | **NO** |  | | |
| R | |  | Employer’s certification shall be revoked when employment is terminated. | 1.6 | 13.0 |
| R | |  | Levels I, II & III whose certifications have been terminated shall be recertified to the former NDT level by a new employer based on examination provide all of the conditions of SNT-TC-1A, Section 13 are met. |
| **Reinstatement** | | | | | |
| **YES** | | **NO** |  | | |
| R | |  | Reinstated to former level, without a new examination, provided all of the following conditions are met:   1. Employer maintained the personnel certification records. 2. Certification did not expire during termination. 3. Reinstated within six (6) months of termination. | 1.6 | 14.0 |